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SHIP NAME:  M.V. GRUAUD LAROSE                                                                       DATE:2024.12.31
MASTER:  _ SERMSAK WANTONG ______
Mooring Line Arrangement 











(Signature) 


(Name) ARNON PROMSAENA
                                                                                                          CHIEF OFFICER

· Judging standard refer to Guideline for hawser ropes condition report 

· Drawing your own ship mooring line arrangement on above patterning

Part 1   Mooring Line Management List 

	Which No.
	Date of Installed
	Date of reversal
	Next intended replacement Date
	Maker
	Type of line
	Break Load (KN)
	Diameter (mm)
	Length(m)

	1
	2024.02.07
	
	2024.08
	N1
	8-strand bbraibddbraided
	892N
	80mm
	200

	2
	2023.03.18
	
	2023.12
	N2
	8-strand
	863 KN
	80mm
	160

	3
	2024.01.10
	2024.04.14
	2024.06
	N3
	8-strand
	892 KN
	80mm
	200

	4
	2021.10.19
	
	2023.12
	N4
	8-strand
	828.9KN
	72mm
	190

	5
	2023.02.02
	2023.06.18
	2023.12
	N5
	8-strand
	774KN
	72mm
	200

	6
	2024.02.07
	
	2024.08
	N6
	8-strand
	892KN
	80mm
	200

	7
	2021.10.19
	
	2024.02
	N7
	8-strand
	1079KN
	80mm
	180

	8
	2024.01.10
	
	2024.06
	N8
	8-strand
	892 KN
	80mm
	200

	9
	2023.03.18
	2023.06.18
	2024.12
	N9
	8-strand
	863 KN
	80mm
	200

	10
	2023.03.18
	2024.01.10
	2024.02
	N10
	8-strand
	1045.6KN
	80mm
	180

	11
	2019.11.04
	2021.10.19
	2024.02
	N11
	8-strand
	719.3KN
	66mm
	170

	12
	2021.10.19
	
	2024.02
	N10
	8-strand
	1045.6KN
	80mm
	190

	13
	
	2021.10.19
	2023.12
	N13
	8-strand
	719.3KN
	66mm
	170

	Spare Mooring Line List

	No.
	Date of supply
	New or used
	Store location
	Maker
	Type of line
	Break Load (KN)
	Diameter (mm)
	Length(m)

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	


Part 2 Inspection Record for Mooring Line 

	Which No.
	Date of inspection

(dd/mm/yy)
	The wear and tear

lever of the outside

layer of the yarn

(Mark lever)
	The weather, wear and tear, and deterioration caused by heat (Mark lever)
	The Check of the part of eye-splice

(Mark lever)
	Actual usage (Months)
	Expect usable

(Months)
	Condition of tail rope and  protecting canvas on the head part

	1
	2024.12.20
	4
	4
	4
	3
	6
	normal

	2
	2024.12.20
	3
	3
	3
	3


	13
	Fair

	3
	2024.12.20
	4
	4
	4
	3
	4
	normal

	4
	2024.12.20
	3
	3
	4
	3
	13
	Fair

	5
	2024.12.20
	4
	4
	4
	3
	17
	Fair

	6
	2024.12.20
	3
	3
	3
	3
	3
	normal

	7
	2024.12.20
	3
	4
	4
	3
	12
	Fair

	8
	2024.12.20
	4
	4
	4
	3
	4
	normal

	9
	2024.12.20
	4
	4
	4
	3
	17
	Fair

	10
	2024.12.20
	3
	3
	4
	3
	13
	Fair

	11
	2024.12.20
	4
	4
	3
	3
	13
	Fair

	12
	2024.12.20
	3
	3
	3
	3
	13
	Fair 

	13
	2024.12.20
	3
	2
	3
	3
	11
	Fair

	
	
	
	
	
	
	
	

	Spare Mooring Line List

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	


Photo condition of mooring lines
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Good condition
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Fair condition





13





3





7





Poor and damage condition
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